Modules | Alphabetical List | Class List | Directories | File List | File Members | GIL Home Page # device_n.hpp File Reference ## Detailed Description Support for color space of N channels and variants. Author: Lubomir Bourdev and Hailin Jin Adobe Systems Incorporated Date: 2005-2007 Last updated on March 8, 2006 `#include "gil_config.hpp"` `#include <boost/type_traits.hpp>` `#include <boost/mpl/range_c.hpp>` `#include <boost/mpl/vector_c.hpp>` Go to the source code of this file.
## Namespaces
namespace | boost
namespace | boost::gil
## Classes
struct | devicen_color_t
| unnamed color More...
struct | devicen_t< 1 >
| unnamed color space of one channel More...
struct | devicen_t< 2 >
| unnamed color space of two channels More...
struct | devicen_t< 3 >
| unnamed color space of three channels More...
struct | devicen_t< 4 >
| unnamed color space of four channels More...
struct | devicen_t< 5 >
| unnamed color space of five channels More...
struct | devicen_layout_t
| unnamed color layout of up to five channels More...
## Functions
template<typename IC>
type_from_x_iterator< planar_pixel_iterator< IC, devicen_t< 2 > > >::view_t | boost::gil::planar_devicen_view (int width, int height, IC c0, IC c1, std::ptrdiff_t rowsize_in_bytes)
| from 2-channel planar data
template<typename IC>
type_from_x_iterator< planar_pixel_iterator< IC, devicen_t< 3 > > >::view_t | boost::gil::planar_devicen_view (int width, int height, IC c0, IC c1, IC c2, std::ptrdiff_t rowsize_in_bytes)
| from 3-channel planar data
template<typename IC>
type_from_x_iterator< planar_pixel_iterator< IC, devicen_t< 4 > > >::view_t | boost::gil::planar_devicen_view (int width, int height, IC c0, IC c1, IC c2, IC c3, std::ptrdiff_t rowsize_in_bytes)
| from 4-channel planar data
template<typename IC>
type_from_x_iterator< planar_pixel_iterator< IC, devicen_t< 5 > > >::view_t | boost::gil::planar_devicen_view (int width, int height, IC c0, IC c1, IC c2, IC c3, IC c4, std::ptrdiff_t rowsize_in_bytes)
| from 5-channel planar data