write_at (3 of 6 overloads)

| Home | Libraries | People | FAQ | More

#### write_at (3 of 6 overloads)

Write a certain amount of data at a specified offset before returning.

    template<
        typename SyncRandomAccessWriteDevice,
        typename ConstBufferSequence,
        typename CompletionCondition>
    std::size_t write_at(
        SyncRandomAccessWriteDevice & d,
        boost::uint64_t offset,
        const ConstBufferSequence & buffers,
        CompletionCondition completion_condition,
        boost::system::error_code & ec);

This function is used to write a certain number of bytes of data to a random access device at a specified offset. The call will block until one of the following conditions is true:

- All of the data in the supplied buffers has been written. That is, the bytes transferred is equal to the sum of the buffer sizes.
- The completion_condition function object returns true.

This operation is implemented in terms of one or more calls to the device's write_some_at function.

###### Parameters

d

  The device to which the data is to be written. The type must support the SyncRandomAccessWriteDevice concept.

offset

  The offset at which the data will be written.

buffers

  One or more buffers containing the data to be written. The sum of the buffer sizes indicates the maximum number of bytes to write to the device.

completion_condition

  The function object to be called to determine whether the write operation is complete. The signature of the function object must be:

      bool completion_condition(
        // Result of latest write_some_at operation.
        const boost::system::error_code& error,

        // Number of bytes transferred so far.
        std::size_t bytes_transferred
      );

  A return value of true indicates that the write operation is complete. False indicates that further calls to the device's write_some_at function are required.

ec

  Set to indicate what error occurred, if any.

###### Return Value

The number of bytes written. If an error occurs, returns the total number of bytes successfully transferred prior to the error.