Generic Image Library: device_n.hpp File Reference

Modules | Alphabetical List | Class List | Directories | File List | GIL Home Page

# device_n.hpp File Reference

## Detailed Description

Support for color space of N channels and variants.

Author:
  Lubomir Bourdev and Hailin Jin
  Adobe Systems Incorporated

Date:
  2005-2009
  Last updated on February 20, 2009

`#include <cstddef>`
`#include "gil_config.hpp"`
`#include "utilities.hpp"`
`#include "metafunctions.hpp"`
`#include <boost/type_traits.hpp>`
`#include <boost/mpl/range_c.hpp>`
`#include <boost/mpl/vector_c.hpp>`

Go to the source code of this file.

## Namespaces

namespace | boost
namespace | boost::gil

## Classes

struct | devicen_color_t
| unnamed color More...
struct | devicen_t< 1 >
| unnamed color space of one channel More...
struct | devicen_t< 2 >
| unnamed color space of two channels More...
struct | devicen_t< 3 >
| unnamed color space of three channels More...
struct | devicen_t< 4 >
| unnamed color space of four channels More...
struct | devicen_t< 5 >
| unnamed color space of five channels More...
struct | devicen_layout_t
| unnamed color layout of up to five channels More...

## Functions

template<typename IC>
type_from_x_iterator < planar_pixel_iterator< IC, devicen_t< 2 > > >::view_t | planar_devicen_view (std::size_t width, std::size_t height, IC c0, IC c1, std::ptrdiff_t rowsize_in_bytes)
| from 2-channel planar data
template<typename IC>
type_from_x_iterator < planar_pixel_iterator< IC, devicen_t< 3 > > >::view_t | planar_devicen_view (std::size_t width, std::size_t height, IC c0, IC c1, IC c2, std::ptrdiff_t rowsize_in_bytes)
| from 3-channel planar data
template<typename IC>
type_from_x_iterator < planar_pixel_iterator< IC, devicen_t< 4 > > >::view_t | planar_devicen_view (std::size_t width, std::size_t height, IC c0, IC c1, IC c2, IC c3, std::ptrdiff_t rowsize_in_bytes)
| from 4-channel planar data
template<typename IC>
type_from_x_iterator < planar_pixel_iterator< IC, devicen_t< 5 > > >::view_t | planar_devicen_view (std::size_t width, std::size_t height, IC c0, IC c1, IC c2, IC c3, IC c4, std::ptrdiff_t rowsize_in_bytes)
| from 5-channel planar data